 

Scrub path: 17-28”

Solution/Rec. Tank: 17 gal

Run time: 3.5 hours

Coverage: 25,543 sq ft/hr

Scrub path: 17-28”

Solution/Rec. Tank: 17 gal

Run time: 3.5 hours

Coverage: 25,543 sq ft/hr

 

Scrub path: 26-34”

Solution/Rec. Tank: 35 gal

Run time: 7 hours

Coverage: 35,500 sq ft/hr

Scrub path: 26-34”

Solution/Rec. Tank: 30 gal

Run time: 5 hours

Coverage: 33,000 sq ft/hr

 

Burnisher: 20” or 27”

Pad Speed: 2000 rpm

Run time: 20”—3 hours

27”—2.5 hours

Coverage:

20”--18,000 sq ft/hr

27”—26,000 sq ft/hr

Scrub path: 34-45”

Solution/Rec. Tank: 68 gal

Run time: 6 hours

Coverage: 50,000 sq ft/hr

 

Sweep Path: 34” or 46”

Hopper capacity:

34”: 2 cu. Ft.

46”: 4 cu. Ft.

Run Time: 34”—4hrs.

46”—6hrs

Coverage:

34”—30,000 sq ft/hr

46”—60,000 sq ft/hr

Burnishing path: 27”

Pad Speed: 1800 rpm

Run time: 4 hours

Coverage: 28,000 sq ft/hr